99-06 Predator PC interface instructions

To save a copy of your original backup file:

1. From this page, download the 99-02 or 03-06 PC interface software.
http://diablosport.com/index.php?module=htmlpages&func=display&pid=17
2. Connect your Predator to the PC using a 9-pin to 9-pin serial cable. If you do not have a serial port on your PC, you can use a USB to serial adapter.

3. Power the Predator up using a 12v 1 amp power supply with a 2.5x5.5mm tip, center positive.

4. From the main menu in the Predator select ‘options’, then ‘PC Communication’.

5. Leave ‘PC Communication’ highlighted, but do not press enter.

6. Open the PC interface software.

7. If using a USB adapter, access your Device Manager to see what COM port it has been assigned to.

8. Set the PC Interface software to the correct COM port under ‘options’, ‘port settings’. If using a serial cable, the default setting of COM1 should work.

9. On the interface software, press the ‘Vehicle backup file’ button under ‘upload from Predator to PC’.

10. You will get a ‘Cry File Name’ window. You can name the file whatever you like, or leave the default name (upload.crg). Do not put any periods in the name of the file.

11. After naming the file, press OK on that window.

12. Now, press enter on ‘PC communications’ on the Predator. The file transfer will happen automatically.

13. There is a status bar in the lower left hand corner that shows what % of the file has been uploaded.

14. Once the file has been saved, the Interface will direct it to a folder in your local disk C: drive.


Sending a custom tune from the PC to Predator:

15. From this page, download the 99-02 or 03-06 PC interface software.
http://diablosport.com/index.php?module=htmlpages&func=display&pid=17
16. Connect your Predator to the PC using a 9-pin to 9-pin serial cable. If you do not have a serial port on your PC, you can use a USB to serial adapter.

17. Power the Predator up using a 12v 1 amp power supply with a 2.5x5.5mm tip, center positive.

18. From the main menu in the Predator select ‘options’, then ‘PC Communication’.

19. Leave ‘PC Communication’ highlighted, but do not press enter.

20. Open the 99-02 PC interface software.

21. If using a USB adapter, access your Device Manager to see what COM port it has been assigned to.

22. Set the PC Interface software to the correct COM port under ‘options’, ‘port settings’. If using a serial cable, the default setting of COM1 should work.

23. On the PC Interface software, press the ‘Performance file’ button under Download from PC to Predator.

24. A new window will open and ask you for the name of the file you wish to send to the Predator. Browse through your PC until you find the file, then click on it one time and press the ‘Open’ button.

25. Then, you’ll press enter on ‘PC Communication’ in the Predator.

26. The file will automatically transfer to the Predator.

27. The Predator will now display ‘Custom tune’ on the main menu instead of ‘Tune it’.

Saving vehicle current tune:

1.Power the Predator up in the vehicle and select ‘Tune it’ from the main menu. Then choose troubleshooting.

2.Go through the disclaimer until you see the next menu and select ‘save current data’.

3.This process will take a few minutes, and when finished you will be asked to cycle the key.

4.Once the vehicles current data is saved, you may unplug the Predator and connect the tool to your PC with the serial cable and power it up.

5.Open the 99-02 or 03-06 PC interface software.

6.On the Predator, choose ‘Options’, then leave ‘PC Communications’ highlighted.

7. Under ‘Upload from Predator to PC, press the ‘Vehicle current file’ button.

8.Name the file or leave the default name. Be sure to use the same file extension if renaming the file.

9.Press OK on the PC, then enter on the tool to begin the file transfer.

10.There is a status bar in the lower left hand corner that shows what % of the file has been uploaded.

11.Once complete, you will see a message stating ‘Upload complete’. The vehicle current tune is now saved to your PC.
If you need any further assistance, please contact our tech support department at 561-908-0040x1.

