Auto Connect is ENABLED.

Legacy Connect is DISABLED.

A tool was found on COM7 at 57600 baud.

XML RPC commands are AVAILABLE.

XML RPC protocol version is 1.60

Tool type = 'Trinity'.

Serial number = '6K3DJ54-1'.

Part number = 'gm_can_gas'.

CROM version = 'gm_can_gas-1r09g 11/07/2012 04:45:10 PM boot3'.

Vehicle VIN = '2G2WC58CX71195332'.

Vehicle Calibration = '12609256'.

Original backup SAVED.

Tool is Married TRUE.

Single user tool FALSE.

Using Class2 Protocol FALSE.

Calibration Updates are NOT supported.

A Calibration Update is NOT required.

XML RPC WILL be used for FRG transfers.

Tune compression is AUTOMATIC.

Tune compression is set to ENABLED.

Tool registration is SUPPORTED.

Tool SUPPORTS multiple ECUs.

Tool reports 2 ECUs.

Multi ECU Backups : 1

Marriage VIN : 2G2WC58CX71195332

 Tool ID : 

 Desc :

